# SWIX VALLATIPS SWIX WAX TIPS FOR

# INFÖR TJEJVASAN "TJEJVASAN"

|  |  |  |
| --- | --- | --- |
| GÄLLANDE LÖRDAG 27.02.2016 |  | FOR SATURDAY February 27 2016 |
|  |  |  |
| Detta vallatips är baserat på väderleksprognoser och testning. TEMPERATURPROGNOS FÖR IMORGONSälen kl. 11.00 -1ºCEvertsberg kl. 12.00 -1ºCOxberg kl. 12.00 0ºCMora kl. 14.00 +2ºCSTRUKTUR***Stenslipade skidor:*** Medium. Kom ihåg att rill ovanpå stenslip ofta ger bättre glid.***Swix Rilljärn:*** 1,00 mm rätt (vals som präglar en rätt struktur på bakändan) (T423/T406).GLID - Alternativ 1:1. Värm in **LF6X**, låt kallna. Värm in en gång till, efter avkylning sickla av med plexisickel och borsta med Swix brons- eller stålborste.
2. Avsluta med Swix blå nylon poleringsborste.

GLID - Alternativ 2 - racing:1. Värm in **HF7X** eller **DHF104BW** (**Svart Marathon)** låt kallna. Värm in en gång till, efter avkylning sickla av med plexi sickel och borsta med Swix brons- eller stålborste.
2. Lägg på **Cera F FC6X**. Använda vallajärn på ca. 165°C. Dra järnet snabbt över belaget. Vänta i ca. 10 min. och borsta bort från belaget med en hästhårs- eller vildsvinsborste.
3. Avsluta med Swix blå nylon poleringsborste.

FÄSTE:1. Rugga fästzonen med slippapper #100 (Swix T330 el. T0011).
2. Lägg på ett lager **VG35** grön grundvax varma in. Låt kalna.
3. Lägg på 4-6 lager **VR40** blå vax. Korka mellan varje lager.
4. Täck med 1-2 lager **VR45** violett vax. Korka lett mellan varje lager.

For dom som startar senare: justera med **VR55N** mjuk violett.Vil du lära dig mer om hur du lägger klister och glidvalla gå in på [swixschool.com](http://www.swixschool.com).LYCKA TILL! |  | These wax tips are based on weather prognoses and testing. TEMPERATURESSälen kl. 11.00 -1ºCEvertsberg kl. 12.00 -1ºCOxberg kl. 12.00 0ºCMora kl. 14.00 +2ºCSTRUCTURE***Stone ground skis:*** Medium structure. Remember to use hand structure on stone ground skis for better glide.***Swix Structure Tools:*** Imprint Tool Roller (T423/T406) “Straight”: 1.00 mm (imprint roller that gives straight structure)GLIDE - Alternative 1:1. Iron in **LF6X**. Let cool off. Iron in once more and let cool off. Scrape off with a Swix Plexi Scraper, and brush with a Swix Bronze or Steel Brush.
2. Finish with the Blue Nylon Polish Brush.

GLIDE - Alternative 2:1. Iron in one layer of **HF7X** or **DHF104BW Black Marathon**. Let cool off. Iron in once more and let cool off. Scrape off with a Swix Plexi Scraper, and brush with a Swix Bronze or Steel Brush.
2. Apply **Cera F FC6X** with an iron temperature of approx. 165°C. Make one fast continuous pass with the iron with a constant pressure – take one side of the groove at the time. Let cool approx. 10 min. Brush up the powder with a stiff, black nylon brush. Continue brushing with a horsehair- or wild boar brush.
3. Finish with the Blue Nylon Polish Brush.

GRIP:1. Sand (rub) the grip zone area with #100 grit silicon sandpaper (Swix T330 or T0011).
2. Iron in one layer of **VG35** Green Base Wax. Let cool off.
3. Apply 4-6 layers of **VR40** Blue Grip Wax. Smooth carefully out between each layer.
4. Cover with 1-2 layers of **VR45** Violet. Smooth carefully out between each layer.

For those who are starting later: apply **VR55N** Soft Violet wax. For more information on how to apply gliders and grip waxes please visit [swixschool.com](http://www.swixschool.com).We wish everybody a nice trip! |