# SWIX FLUOR FRITT VALLATIPS ÖPPETSPÅR MÅNDAG

## GÄLLANDE MÅNDAG 25.02.2019

Detta vallatips är baserat på väderleksprognoser och testning.

## TEMPERATURPROGNOS

Sälen kl. 07.00 0ºC

Evertsberg kl. 10.00 +1ºC

Mora kl. 13.00 +5ºC

## STRUKTUR

**Stenslipade skidor:** Fin till medium. Kom ihåg att rill ovanpå stenslip ofta ger bättre glid.

**SWIX Rilljärn:** 1,00 mm rätt struktur (T423 alt. T401).

## GLID

1. Värm in lager med **CH6X** låt kallna sickla och borst för slitstyrkan.
2. Spraya på **CH8XL Liquid,** låt torka. Applicera vid en temperatur över 10°C. Var noga med att det torkar minst 15 minuter.
3. Avsluta med SWIX blå nylon poleringsborste.

## FÄSTE

1. Rugga fästzonen med slippapper #100 (SWIX T330 el. T0011).
2. Lägg på ett lager **KB20** grönt grundklister. Låt kalna.
3. Lägg ett lager **KX35** Lila klister.
4. Toppa med ett lager **KN44** Nero klister.

## SKIN-SKIDOR

Skall Du åka med **skin-skidor**, rengör först med **N16 Skin Cleaner**. därefter impregnerar du skin-ytan med **N15 Skin Care.**

Detta var dagens vallarekommendation inför Vasaloppsveckan.

## LYCKA TILL!

# SWIX FLUOR FREE WAX TIPS ÖPPETSPÅR MONDAY

## FOR MONDAY FEBRUARY 25, 2019

These wax tips are based on weather prognoses and testing.

## TEMPERATURES

Sälen kl. 07.00 0ºC

Evertsberg kl. 10.00 +1ºC

Mora kl. 13.00 +5ºC

## STRUCTURE

**Stone ground skis:** Fine to medium structure. Remember to use hand structure on stone ground skis for better glide.

**SWIX Structure Tool:** 1.0 mm linear structure (T423 or T401 tool).

## GLIDE

1. Iron in one layer of **CH6X** Let cool off. Iron in once more and let cool off. Scrape off with a Plexi Scraper, and brush with a SWIX Bronze or Steel Brush.
2. Spray on **CH8XL** **Liquid** and let dry for at least 15 minutes. Apply the product in temperatures above 10°C. To obtain the best performance it’s important to allow the wax film to dry entirely.
3. Finish with the SWIX Blue Nylon Polish Brush.

## GRIP

1. Sand (rub) the grip zone area with #100 grit silicon sandpaper (SWIX T330 or T0011).
2. Apply a thin layer of **KB20** Green Base Klister spray. Let dry.
3. Apply one layer of **KK35** Violet klister. Smooth carefully out.
4. Top with a layer of **KN44** Nero klister. Smooth carefully out.

## SKIN SKIS

If you are using **skis with integrated skins** we recommend to clean the skins with **N16 Skin Cleaner** and then use **N15 Skin Care** to improve the skins glide properties.

## We wish everybody a nice trip!