# SWIX FLUOR FRITT VALLATIPS INFÖR VASALOPPET

## GÄLLANDE SÖNDAG 03.03.2019

Detta vallatips är baserat på väderleksprognoser och testning.

## TEMPERATURPROGNOS

Sälen kl. 08.00 -6ºC

Evertsberg kl. 10.00 -4ºC

Mora kl. 13.00 -2ºC

## STRUKTUR

**Stenslipade skidor:** Fin till medium. Kom ihåg att rill ovanpå stenslip ofta ger bättre glid.

**SWIX Rilljärn:** 1,00 mm rätt struktur (T423 alt. T401).

## GLID

1. Värm in lager med **CH6X** låt kallna sickla och borst för slitstyrkan.
2. Spraya på **CH8XL Liquid,** låt torka. Applicera vid en temperatur över 10°C. Var noga med att det torkar minst 15 minuter.
3. Avsluta med SWIX blå nylon poleringsborste.

## FÄSTE

1. Rugga fästzonen med slippapper #100 (SWIX T330 el. T0011).
2. Värm på ett lager **VG35** grönt grundvax. Låt kalna
3. Värm in ett lager **V30** blå burk.
4. Lägg 4-6 tunna lager **V45** lila burk.
5. Kan vara bra att ta med på turen**.**

**V50** vid bakhalt, skrapa och kloss

## SKIN-SKIDOR

Skall Du åka med **skin-skidor**, rengör först med **N16 Skin Cleaner**. därefter impregnerar du skin-ytan med **N15 Skin Care.**

Vi återkommer med en uppdaterad prognos på fäste imorgon.

## LYCKA TILL!

# SWIX FLUOR FREE WAX TIPS **FOR VASALOPPET**

## FOR SUNDAY MARCH 03, 2019

These wax recommendations are based on weather prognoses and testing.

## TEMPERATURES

Sälen kl. 08.00 -6ºC

Evertsberg kl. 10.00 -4ºC

Mora kl. 13.00 -2ºC

## STRUCTURE

**Stone ground skis:** Fine to medium structure. Remember to use hand structure on stone ground skis for better glide.

**SWIX Structure Tool:** 1.0 mm linear structure (T423 or T401 tool).

## GLIDE

1. Iron in one layer of **CH6X** Let cool off. Iron in once more and let cool off. Scrape off with a Plexi Scraper, and brush with a SWIX Bronze or Steel Brush.
2. Spray on **CH8XL** **Liquid** and let dry for at least 15 minutes. Apply the product in temperatures above 10°C. To obtain the best performance it’s important to allow the wax film to dry entirely.
3. Finish with the SWIX Blue Nylon Polish Brush.

## GRIP

1. Sand (rub) the grip zone area with #100 grit silicon sandpaper (Swix T330 or T0011).
2. Iron in one layer of **VG35** Green Base Binder. Let cool off.
3. Iron in one layer of **V30** Blue Grip Wax. Let cool of.
4. Apply 4-6 thin layers of **V45** Purpel Grip Wax. Smooth carefully out between each layer.
5. Can be good to bring along the tour.

**V50** if it´s slippery, scraper and block

## SKIN SKIS

If you are using **skis with integrated skins** we recommend to clean the skins with **N16 Skin Cleaner** and then use **N15 Skin Care** to improve the skins glide properties.

## We wish everybody a nice trip!